* 41 a -

On each annual inspection the mounting studs on the canopy lifting frame must be checked for wear and, if necessary, be reconditioned in compliance with Technical Note No. 303 – 18.